While recording it is possible to have access to different signals which are recorded. Accessing the signals is done via TCP/IP protocol. You have access to: the two rotating buffers which are used for the online processing. the continuous signals of all recorded channels the current value of all recorded channels the current digital trigger can be exported You find example applications for LabView called e.g. GetRawData.vi which shows how to access the TCP/IP port and extract the signals. For the TCP/IP communication port 6339 is used. The command sent to IMAGO Record program is the string: GETRAW. Coming back is a string with 4 bytes specifying the size if the data package and the data. Tabs are used to separate the float numbers, Return is the column separator. The data are sent from the left window of IMAGO Record. The information of the right window is directly sent afterwards, once more starting with 4 bytes specifying the size of the data package and the data.