After leaving the online processing windows, an Excel file can be written with all necessary results. If you do not want to write a file, press Cancel. The file contains a table with all mean plots, standard deviations and has separate columns for rectified and not rectified signals. In addition, the signal amplitudes between the cursor pairs are written. The file extension is the number of the trigger condition. E.g. my_data.bin will generate files called my_data.007 for the trigger number 7. If only one digital trigger value is available, the extension my_data.xls is used. The size of the text file depends on the window size, the sample frequency and the number of recorded channels. E.g. a file with 6 channels, 5kHz sample frequency and a window size of 150ms will generate a file with 5000(Samples / s) * 0,15 = 750 lines and 6 * 3 (mean +- STD) * 2 (rectified, not rectified) = 36 columns.