The Remore Control function can be used to automize the start and the end of a recording. Press the Remote Control button to see all available settings. The Remote Control button is available when Measurement is pressed. E.g. you want to record 30 seconds of a trial with a repetition period of 2 minutes starting 1 minute after the begin of the trial. Insert 30 seconds as record time [seconds], 120 seconds as waiting time [seconds] and the number of repetitions. If the number of repetitions is > 0, the setting will be repeated. If the order of recording and pause is not symmetrical, input the desired record and pause times into single lines, each with repetition 0. To define an initial delay of 1 minute, insert 60 seconds as start delay [seconds] Insert a basic filename without extension. An index will be automatically added and incremented for every recorded signal. If you e.g. enter test as basic filename, the first recorded signal will be stored as test_1.bin, the second one as test_2.bin To activate the Remote Control function, switch from Off to Active and press Continue. The current time will be used to calculate the recording and pause times. The entries of the Remote Control are also written to Setup file. The setting will be Off after loading and must be activated to start. Press Clear to remove all entries from the list, press Cancel to leave Remote Control without changing anything. Press Continue to accept the changes and close the window.