After the selection of all necessary digital triggers, every single data piece can be reviewed and selected for the final online processing. This can be done manually or automatically. Pressing Continue will ask if the selected number of curves is OK and if you want to save the selection to the *.TRG file. This marks the bad signals in the TRG file as invalid. If a further processing is done with Process Master or the file is once more processed with the Online processing of IMAGO Record, only the valid signals will be used. Manual Selection Select the channel to view. Press OK (F2) or Skip (F3) to select the shown signal. Move foreward and backward with the slider below the graph. If a signal piece was already selected, the LED is green. If a signal piece was skipped, the LED is red. Press the Always button beside the OK button to accept all signal pieces of the shown digital trigger condition. Press the Always button beside the Skip button to skip all signal pieces of the shown digital trigger condition. Press the Always button beside the button All triggers from all conditions to select all signal pieces of all digital trigger conditions for this run and for the next runs. To disable the Always buttons, go to the menu bar and deactivate Imago -> Always active A third pair of purple cursors can be used to test the amplitudes of a reflex without changing the position of the other cursors which are relevant for the results. Visual Selection Pressing the button Visual Selection opens a window which shows all available signals with the same x- and y-axis. To disable bad signals, press the left mouse button to select the signal. Each curve hat a cursor which moves to the mouse location if you click. If you click to the cursor, the curve is highlighted which means the signal will not be used for the proceeding online processing. Click once more to the same cursor to de-select it. Press OK to accept your selection or Cancel. Automatic Selection Select the channel to view. Check the position of the H-Cursors. The signal between these cursors is used for the automatic function. Press the Automatic button. Select either Reflex Size or Amplitude Selection. Search all signals / Search already selected signals If you start the Automatic function the first time, select Search all signals. All signals will be qualified no matter if they are selected or not. You can fine-tune a selection with a second run of the Automatic function. You can e.g. select a different channel and once do an automatic selection. Select the setting: Search already selected signals so that only signals are qualified which have already been selected. Automatic Function: Reflex Size Input the maximum and minimum allowed reflex size and press Start Automatic. The maximum and minimum is searched for every signal piece between the H-Cursors. The reflex size is calculated as maximum - minimum and compared with the allowed maximum and minimum. Afterwards, a messagebox appears showing the number of selected signals. Accept this selection or continue with the selection. The automatic selection will stay activated and can be manually adjusted if necessary. Automatic Function: Amplitude Selection Input the maximum and minimum allowed amplitude of the selected channel and press Start Automatic. For each signal piece the mean amplitude between the H-Cursors is calculated. This value is compared with the allowed maximum and minimum amplitude value. Afterwards, a messagebox appears showing the number of selected signals. Accept this selection or continue with the manual selection. The automatic selection will stay activated and can be manually adjusted if necessary.