For the data processing a different file format is needed which is called Channel Format. This format contains all information about the channels. Directly converted Channel Format files have the extention *.C00. The 00 represents the first step of the signal processing. After the next step, the file will be renamed into *.C01 and so on. Each channel format file has an additional trigger information file with the same name and the extension *.T00 / *.T01 / ... The trigger file is automatically loaded with the Channel Format file.