The Superimposed Traces window allows the view of a combination of all available signals. On the right side you find a list of all possible signals and all possible trigger conditions. You can easily generate plots which show differences of a channel between the trigger conditions. You can choose a different color for each plot. The color is selected with the color field above the Signal Selection table. Normally the plot shows the Mean of the signal and the mean is calculated from all recorded and selected data pieces, not only from a circular buffer. It is also possible to show Mean +- standard deviation. Click on Mean +- STD to change the view. If rectified is pressed, the signal pieces are first rectified before the mean is calculated. The units used in this window are all physical units. Use therefore the calibration values in the instruments to define the equivalent to 1V to a physical unit, e.g. 1V at the A/D converter = 5mV electrical signal before amplification. Use the Print button to get a good documentation of the selected channels. All selections and colors can be stored in a file. Press Save Setup to store the file and Load Setup to re-load it. The filename of the stored file can be combined with the setting which is stored in IMAGO Record. After the selection and saving the setup in the online processing window, go back to IMAGO Record and save the complete setting with the reference to the online processing file. Press New Selection to return to the selection of digital triggers and signal pieces. This is useful if you want to process one trigger condition after each other with slightly different cursor positions. This can be done without leaving the online processing. Press Refresh to re-calculate the reflex sizes and delays. Especially when moving the cursors this might be necessary. After pressing Save+Repeat or Save+Exit a file selection box appears and you can choose a name to write text files with all relevant information for further examinations with Excel. The file extension will be defined automatically and represents the digital trigger number. Choosing Save+Repeat will not exit the processing window so that you have the possibility to do some changes and once more save the result without leaving the window.