IMAGO-signal processing is done in several steps: Convert The BIN file is converted to floating point numbers. In addition, voltages are converted to physical units. Trigger With the Trigger Generation module triggers can be set at file positions which are needed for the signal processing. The Trigger Signal Cut module uses these trigger positions to define signal pieces with a defined length. These signal pieces are the heart of the complete signal processing. Selection After the signal piece generation each signal piece can be selected manually or automatically to eliminate wrong signal pieces. Save The signal pieces are saved in the Channel Format. This ensures that you need to define the signal pieces only once. The file extension will be *.C01 Specific Processing With the *.C01 file the necessary processing is done. Export The extracted parameters can be stored in a text file to load into Excel or other statistic programs for further steps.