The BioAmp amplifier can be used to amplify EEG or EMG signals. This amplifier has no direct interaction with IMAGO. Therefore, you need to define your setup for the BioAmp amplifier to program the hardware and in addition use the Channel Definition Instrument to define the channel names and the calibration values for all channels. Since Windows 2000, LabView can not any more directly access the parallel port. Therefore, an additional device driver must be installed. It is available in the full version in the directory Imago\utilities\AccessHW or in the Install version in the directory programs\Imago\Record\Utilities\AccessHW. Run the setup.exe.