Channel Compare provides the possibility to calculate results based on the difference of two channels. Select the channels and the trigger condition. The differences for all signal pieces are shown in a separate window. In the table below the results for all signal pieces are shown. These results are based on the position of the cursors. To generate files for all trigger conditions, press Save+Repeat button. After saving the file, you can choose the next trigger condition of channel setting and save again. After pressing Save+Exit a file selection box appears and you can choose a name to write a text file with the content of the shown table for further examination. The file extension will be defined automatically and represents the digital trigger number.